; COMP_MDM_USB.inf
;
; Installation of usb modem driver description file (INF) for Motorola V878 and V690 
; phones.
;
; Copyright (c) 2004 by Motorola, Inc. 

[Manufacturer]
%Motorola% = Motorola

[Motorola]
%Moto%=Moto, USB\VID_067B&PID_2303

[SourceDisksNames]
1 = %Motorola.Disk%,,,

[SourceDisksFiles]
SER9PL.SYS = 1
SERSPL.VXD = 1
ser2pl.sys = 1
COMP_MDM.INF = 1

[DestinationDirs]
USB2SER.Files.Ext = 11
Files.Inf = 17
DefaultDestDir = 12

[Files.Inf]
COMP_MDM.INF

[Moto_install]
;Windows98_ME

[Version]
Signature="$Windows 95$"
Class=USB
SetupClass=BASE
provider=%Motorola%


[Moto]
CopyFiles=USB2SER.Files.Ext, Files.Inf
AddReg=USB2SER.AddReg

[USB2SER.AddReg]
HKR,,DevLoader,0,*ntkern
HKR,,NTMPDriver,,SER9PL.SYS

[USB2SER.Files.Ext]
SER9PL.SYS
SERSPL.VXD

;========================================================================
;
;========================================================================
[Moto_Install.NTx86]
;Windows2000

[Version]
Signature="$Windows NT$"
Class=Modem
ClassGuid={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Motorola%
LayoutFile=layout.inf
DriverVer=05/05/2004,1.5.0.1

[Moto.NT]
CopyFiles=Moto.NT.Copy, Files.Inf
Include=COMP_MDM.inf
Needs=Moto1

[Moto.NT.HW]
AddReg=Moto.NT.HW.AddReg

[Moto.NT.Copy]
ser2pl.sys

[Moto.NT.HW.AddReg]
HKR,,"LowerFilters",0x00010000,"ser2pl"

[Moto.NT.Services]
AddService=ser2pl, 0x00000000, LowerFilter_Service_Inst
	
[LowerFilter_Service_Inst]
DisplayName=%USBFilterString%
ServiceType= 1
StartType  = 3
ErrorControl = 0
ServiceBinary = %12%\ser2pl.sys

;========================================================================
;
;========================================================================
[Strings]
Motorola = "Motorola"
Motorola.Disk = "USB-Serial Disk"
Moto = "Motorola Comp Modem"
USBFilterString="USB Filter Driver"

